**Additional equipment**

**Fire Protection - Stacking door HERO**

**EI2 90 C2 Sa**

**- For low lintel heights, also available as telescopic lifting door (only for Sa)**

Surface coating:  
Wet coating - color hues according to RAL, DB or NCS

Electrical options:   
Self-holding (pulse control) with additional safety equipment possible, timed closing

Smoke switches:  
Also available in RAL coated version and flush-mounted version

for suspended ceilings and false ceilings (also coated)

Command devices:  
Key switch, triple push-button, radio, pull switch,

Release buttons:   
Surface-mounted underglass with reset, flush-mounted underglass with reset

Other high quality push-button/reset combinations (incl. stainless steel etc.) possible on request

Flaps for invisible fire protection:  
Side niche flaps (one-sided or double-sided)

Ceiling flap (in conjunction with flap control for controlled flap course)

Flap design versions: ALU blank (standard), wet-coated, wallpapered or prepared for a later, builder-owner provided coating (wood, tiles, etc.).

Automated guided vehicle systems (AGVS):  
Automated (driverless) transport systems also possible with special controls